,Light Engine##OTHER##,Drive Current##OTHER##,LED Colour##OTHER##,Fixing Accessories##OTHER##,Model##OTHER##,Colour##OTHER##,Finish Material##OTHER##,Has Concrete-in Box##OTHER##,Control IES##OTHER##,MFG_LightSource##OTHER##,MFG_TemperatureRating##OTHER##,MFG_Wattage##ELECTRICAL_WATTAGE##WATTS
E3 350mA 2200K Black Spring Clips,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),Spring Clips,LD175-E3-350/LW22/Black/SC,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2200K Black Concrete-in Box,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),Concrete-in Box,LD175-E3-350/LW22/Black/CB,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2200K White Spring Clips,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),Spring Clips,LD175-E3-350/LW22/White/SC,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2200K White Concrete-in Box,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),Concrete-in Box,LD175-E3-350/LW22/White/CB,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2200K RAL TBD Spring Clips,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),Spring Clips,LD175-E3-350/LW22/RAL/SC,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2200K RAL TBD Concrete-in Box,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),Concrete-in Box,LD175-E3-350/LW22/RAL/CB,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2200K Polished Stainless Steel Spring Clips,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),Spring Clips,LD175-E3-350/LW22/Polished & Passivated 316 Stainless Steel/SC,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2200K Polished Stainless Steel Concrete-in Box,E3 LED Engine,350mA (5W LED),Super Warm White (2200K),Concrete-in Box,LD175-E3-350/LW22/Polished & Passivated 316 Stainless Steel/CB,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2700K Black Spring Clips,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),Spring Clips,LD175-E3-350/LW27/Black/SC,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2700K Black Concrete-in Box,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),Concrete-in Box,LD175-E3-350/LW27/Black/CB,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2700K White Spring Clips,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),Spring Clips,LD175-E3-350/LW27/White/SC,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2700K White Concrete-in Box,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),Concrete-in Box,LD175-E3-350/LW27/White/CB,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2700K RAL TBD Spring Clips,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),Spring Clips,LD175-E3-350/LW27/RAL/SC,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2700K RAL TBD Concrete-in Box,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),Concrete-in Box,LD175-E3-350/LW27/RAL/CB,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2700K Polished Stainless Steel Spring Clips,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),Spring Clips,LD175-E3-350/LW27/Polished & Passivated 316 Stainless Steel/SC,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 2700K Polished Stainless Steel Concrete-in Box,E3 LED Engine,350mA (5W LED),Extra Warm White (2700K),Concrete-in Box,LD175-E3-350/LW27/Polished & Passivated 316 Stainless Steel/CB,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 3000K Black Spring Clips,E3 LED Engine,350mA (5W LED),Warm White (3000K),Spring Clips,LD175-E3-350/LW30/Black/SC,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 3000K Black Concrete-in Box,E3 LED Engine,350mA (5W LED),Warm White (3000K),Concrete-in Box,LD175-E3-350/LW30/Black/CB,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 3000K White Spring Clips,E3 LED Engine,350mA (5W LED),Warm White (3000K),Spring Clips,LD175-E3-350/LW30/White/SC,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 3000K White Concrete-in Box,E3 LED Engine,350mA (5W LED),Warm White (3000K),Concrete-in Box,LD175-E3-350/LW30/White/CB,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 3000K RAL TBD Spring Clips,E3 LED Engine,350mA (5W LED),Warm White (3000K),Spring Clips,LD175-E3-350/LW30/RAL/SC,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 3000K RAL TBD Concrete-in Box,E3 LED Engine,350mA (5W LED),Warm White (3000K),Concrete-in Box,LD175-E3-350/LW30/RAL/CB,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 3000K Polished Stainless Steel Spring Clips,E3 LED Engine,350mA (5W LED),Warm White (3000K),Spring Clips,LD175-E3-350/LW30/Polished & Passivated 316 Stainless Steel/SC,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 3000K Polished Stainless Steel Concrete-in Box,E3 LED Engine,350mA (5W LED),Warm White (3000K),Concrete-in Box,LD175-E3-350/LW30/Polished & Passivated 316 Stainless Steel/CB,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 4000K Black Spring Clips,E3 LED Engine,350mA (5W LED),White (4000K) - on request,Spring Clips,LD175-E3-350/LW40/Black/SC,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 4000K Black Concrete-in Box,E3 LED Engine,350mA (5W LED),White (4000K) - on request,Concrete-in Box,LD175-E3-350/LW40/Black/CB,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 4000K White Spring Clips,E3 LED Engine,350mA (5W LED),White (4000K) - on request,Spring Clips,LD175-E3-350/LW40/White/SC,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 4000K White Concrete-in Box,E3 LED Engine,350mA (5W LED),White (4000K) - on request,Concrete-in Box,LD175-E3-350/LW40/White/CB,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 4000K RAL TBD Spring Clips,E3 LED Engine,350mA (5W LED),White (4000K) - on request,Spring Clips,LD175-E3-350/LW40/RAL/SC,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 4000K RAL TBD Concrete-in Box,E3 LED Engine,350mA (5W LED),White (4000K) - on request,Concrete-in Box,LD175-E3-350/LW40/RAL/CB,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 4000K Polished Stainless Steel Spring Clips,E3 LED Engine,350mA (5W LED),White (4000K) - on request,Spring Clips,LD175-E3-350/LW40/Polished & Passivated 316 Stainless Steel/SC,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 4000K Polished Stainless Steel Concrete-in Box,E3 LED Engine,350mA (5W LED),White (4000K) - on request,Concrete-in Box,LD175-E3-350/LW40/Polished & Passivated 316 Stainless Steel/CB,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 5000K Black Spring Clips,E3 LED Engine,350mA (5W LED),Cool White (5000K),Spring Clips,LD175-E3-350/LW50/Black/SC,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 5000K Black Concrete-in Box,E3 LED Engine,350mA (5W LED),Cool White (5000K),Concrete-in Box,LD175-E3-350/LW50/Black/CB,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 5000K White Spring Clips,E3 LED Engine,350mA (5W LED),Cool White (5000K),Spring Clips,LD175-E3-350/LW50/White/SC,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 5000K White Concrete-in Box,E3 LED Engine,350mA (5W LED),Cool White (5000K),Concrete-in Box,LD175-E3-350/LW50/White/CB,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 5000K RAL TBD Spring Clips,E3 LED Engine,350mA (5W LED),Cool White (5000K),Spring Clips,LD175-E3-350/LW50/RAL/SC,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 5000K RAL TBD Concrete-in Box,E3 LED Engine,350mA (5W LED),Cool White (5000K),Concrete-in Box,LD175-E3-350/LW50/RAL/CB,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 5000K Polished Stainless Steel Spring Clips,E3 LED Engine,350mA (5W LED),Cool White (5000K),Spring Clips,LD175-E3-350/LW50/Polished & Passivated 316 Stainless Steel/SC,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,0,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 350mA 5000K Polished Stainless Steel Concrete-in Box,E3 LED Engine,350mA (5W LED),Cool White (5000K),Concrete-in Box,LD175-E3-350/LW50/Polished & Passivated 316 Stainless Steel/CB,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,1,LightGraphix_IES_LD175 : LD175-E3-350-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,4.2
E3 500mA 2200K Black Spring Clips,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),Spring Clips,LD175-E3-500/LW22/Black/SC,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2200K Black Concrete-in Box,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),Concrete-in Box,LD175-E3-500/LW22/Black/CB,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2200K White Spring Clips,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),Spring Clips,LD175-E3-500/LW22/White/SC,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2200K White Concrete-in Box,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),Concrete-in Box,LD175-E3-500/LW22/White/CB,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2200K RAL TBD Spring Clips,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),Spring Clips,LD175-E3-500/LW22/RAL/SC,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2200K RAL TBD Concrete-in Box,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),Concrete-in Box,LD175-E3-500/LW22/RAL/CB,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2200K Polished Stainless Steel Spring Clips,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),Spring Clips,LD175-E3-500/LW22/Polished & Passivated 316 Stainless Steel/SC,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2200K Polished Stainless Steel Concrete-in Box,E3 LED Engine,500mA (7W LED),Super Warm White (2200K),Concrete-in Box,LD175-E3-500/LW22/Polished & Passivated 316 Stainless Steel/CB,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2700K Black Spring Clips,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),Spring Clips,LD175-E3-500/LW27/Black/SC,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2700K Black Concrete-in Box,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),Concrete-in Box,LD175-E3-500/LW27/Black/CB,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2700K White Spring Clips,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),Spring Clips,LD175-E3-500/LW27/White/SC,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2700K White Concrete-in Box,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),Concrete-in Box,LD175-E3-500/LW27/White/CB,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2700K RAL TBD Spring Clips,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),Spring Clips,LD175-E3-500/LW27/RAL/SC,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2700K RAL TBD Concrete-in Box,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),Concrete-in Box,LD175-E3-500/LW27/RAL/CB,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2700K Polished Stainless Steel Spring Clips,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),Spring Clips,LD175-E3-500/LW27/Polished & Passivated 316 Stainless Steel/SC,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 2700K Polished Stainless Steel Concrete-in Box,E3 LED Engine,500mA (7W LED),Extra Warm White (2700K),Concrete-in Box,LD175-E3-500/LW27/Polished & Passivated 316 Stainless Steel/CB,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 3000K Black Spring Clips,E3 LED Engine,500mA (7W LED),Warm White (3000K),Spring Clips,LD175-E3-500/LW30/Black/SC,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 3000K Black Concrete-in Box,E3 LED Engine,500mA (7W LED),Warm White (3000K),Concrete-in Box,LD175-E3-500/LW30/Black/CB,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 3000K White Spring Clips,E3 LED Engine,500mA (7W LED),Warm White (3000K),Spring Clips,LD175-E3-500/LW30/White/SC,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 3000K White Concrete-in Box,E3 LED Engine,500mA (7W LED),Warm White (3000K),Concrete-in Box,LD175-E3-500/LW30/White/CB,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 3000K RAL TBD Spring Clips,E3 LED Engine,500mA (7W LED),Warm White (3000K),Spring Clips,LD175-E3-500/LW30/RAL/SC,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 3000K RAL TBD Concrete-in Box,E3 LED Engine,500mA (7W LED),Warm White (3000K),Concrete-in Box,LD175-E3-500/LW30/RAL/CB,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 3000K Polished Stainless Steel Spring Clips,E3 LED Engine,500mA (7W LED),Warm White (3000K),Spring Clips,LD175-E3-500/LW30/Polished & Passivated 316 Stainless Steel/SC,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 3000K Polished Stainless Steel Concrete-in Box,E3 LED Engine,500mA (7W LED),Warm White (3000K),Concrete-in Box,LD175-E3-500/LW30/Polished & Passivated 316 Stainless Steel/CB,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 4000K Black Spring Clips,E3 LED Engine,500mA (7W LED),White (4000K) - on request,Spring Clips,LD175-E3-500/LW40/Black/SC,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 4000K Black Concrete-in Box,E3 LED Engine,500mA (7W LED),White (4000K) - on request,Concrete-in Box,LD175-E3-500/LW40/Black/CB,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 4000K White Spring Clips,E3 LED Engine,500mA (7W LED),White (4000K) - on request,Spring Clips,LD175-E3-500/LW40/White/SC,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 4000K White Concrete-in Box,E3 LED Engine,500mA (7W LED),White (4000K) - on request,Concrete-in Box,LD175-E3-500/LW40/White/CB,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 4000K RAL TBD Spring Clips,E3 LED Engine,500mA (7W LED),White (4000K) - on request,Spring Clips,LD175-E3-500/LW40/RAL/SC,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 4000K RAL TBD Concrete-in Box,E3 LED Engine,500mA (7W LED),White (4000K) - on request,Concrete-in Box,LD175-E3-500/LW40/RAL/CB,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 4000K Polished Stainless Steel Spring Clips,E3 LED Engine,500mA (7W LED),White (4000K) - on request,Spring Clips,LD175-E3-500/LW40/Polished & Passivated 316 Stainless Steel/SC,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 4000K Polished Stainless Steel Concrete-in Box,E3 LED Engine,500mA (7W LED),White (4000K) - on request,Concrete-in Box,LD175-E3-500/LW40/Polished & Passivated 316 Stainless Steel/CB,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 5000K Black Spring Clips,E3 LED Engine,500mA (7W LED),Cool White (5000K),Spring Clips,LD175-E3-500/LW50/Black/SC,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 5000K Black Concrete-in Box,E3 LED Engine,500mA (7W LED),Cool White (5000K),Concrete-in Box,LD175-E3-500/LW50/Black/CB,Paint Finish Black (RAL 9005),LightGraphix_Finish_PowderCoat_Black,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 5000K White Spring Clips,E3 LED Engine,500mA (7W LED),Cool White (5000K),Spring Clips,LD175-E3-500/LW50/White/SC,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 5000K White Concrete-in Box,E3 LED Engine,500mA (7W LED),Cool White (5000K),Concrete-in Box,LD175-E3-500/LW50/White/CB,Paint Finish White (RAL 9016),LightGraphix_Finish_PowderCoat_White,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 5000K RAL TBD Spring Clips,E3 LED Engine,500mA (7W LED),Cool White (5000K),Spring Clips,LD175-E3-500/LW50/RAL/SC,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 5000K RAL TBD Concrete-in Box,E3 LED Engine,500mA (7W LED),Cool White (5000K),Concrete-in Box,LD175-E3-500/LW50/RAL/CB,Paint Finish RAL (TBD),LightGraphix_Finish_PowderCoat_RAL (TBD),1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 5000K Polished Stainless Steel Spring Clips,E3 LED Engine,500mA (7W LED),Cool White (5000K),Spring Clips,LD175-E3-500/LW50/Polished & Passivated 316 Stainless Steel/SC,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,0,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
E3 500mA 5000K Polished Stainless Steel Concrete-in Box,E3 LED Engine,500mA (7W LED),Cool White (5000K),Concrete-in Box,LD175-E3-500/LW50/Polished & Passivated 316 Stainless Steel/CB,Polished & Passivated 316 Stainless Steel,LightGraphix_Finish_Stainless Steel_Polished,1,LightGraphix_IES_LD175 : LD175-E3-500-LW30-WIDE,NICHIA E3 LED,-20°C to 55°C,6.0
